Rock Imager 2 Specifications

**Specifications**

**Configurations**  
- Visible bright field only  
- Dual light path: Separate visible and UV  
- Single light path: visible and UV combined

**Plate Capacity**  
Choice of one adapter with purchase  
SBS adapter: 2 SBS plates. (can accommodate LCP thin glass plate with plate supporter)  
Linbro adapter: 1 Linbro plate.

**Compatible Plate Types**  
SBS standard microplate (127.8 x 85.5 mm x 14.4 mm)  
Hampton Microbatch  
LCP thin glass with adapter (127.8 x 85.5 mm x 1 mm) (Thin glass plate holder is available for use without adapters)  
Linbro Plate(150 mm x 108 mm x 22 mm) with specific adapter

**Physical Dimensions**

**Rock Imager 2**

* Depth: 354 mm (13.9 in.)
* Width: 419 mm (16.5 in.)
* Height: 580 mm (22.8 in.)
* Weight: 23kg (51 lbs)
* Shipping weight : 55 kg (121 lbs)

**Electrical**

* Robotics: 100-240 V, 50-60 Hz, 150 W max, 1-phase [Fuse : 6.3A]
* Computer: 375 W max, 1-phase