NT8 LCP

<http://www.formulatrix.com/demosite/liquid-handling/products/nt8/index.html#tabbed-nav=tab3>

**LCP Head Attachment**

The optional LCP dispensing attachment is able to dispense LCP drops of 25 nL - 200 nL. The dispenser holds an 8 mm barrel syringe while a sensor ensures the syringe is properly mounted before dispensing. Dispensing both lipid and well solution to a complete 96-drop LCP plate takes fewer than 5 minutes.

**LCP Mixer**

The LCP dispensing option includes a lipid mixer which attaches to the deck of the NT8. The mixer is controlled by software to guarantee that the right number of mixing cycles are applied to the lipid syringe.

**LCP Auto -Calibration**

The LCP option includes a fully automatic system for calibrating the lipid syringe, ensuring that the syringe tip is centered to within 50 µM.